BSW6540_Readme.txt

SnP Filename convention:

BSWxxxx_Temperature_VDD_VIH_VIL_ONpath_DataFormat

Example file:

BSW6540_25C_5V_3.3V_0V_RF1_RI.s3p

BSWxxxx = Product number
Temperature = Temperature of DUT when measured
VDD = VDD of test iteration
VIH = Logic High Control Voltage Level
VIL = Logic Low Control Voltage Level
ONpath = RFC port to create a through path
DataFormat = RI(Real-Imaginary) / LA (LogMag-Angle)
____________________________________
VNA port defintions:
Port 1 = RFC
Port 2 = RF1
Port 3 = RF2
Port 4 = RF3
Port 5 = RF4
____________________________________
Measurement Date = 2026-05-06
Engineer = MHY (R&D2)